PART 1 – GENERAL
1.01 Section Includes
A. Sprayed cellulose acoustical finish system. (09 83 16)

1.02 Related Items
A. Clips, hangers, supports, sleeves and other attachments to spray bases are to be placed by other trades prior to the application of the acoustical finish system.
B. Ducts, piping, conduit or other suspended equipment shall not be positioned until after the application of the acoustical finish system.
C. Roof penetrations to be installed prior to application.

1.03 Quality Assurance
A. Manufacturer must be in compliance with the 2009-2021 International Building Code.
B. Manufacturer must be ISO 9001:2015 Certified.
C. Manufacturer shall have a minimum 10-year successful performance history of producing and installation of spray-applied cellulose on similar projects
D. Applicator: Licensed by manufacturer.
E. Mock-up: Apply a 100 square foot representative sample to be reviewed by the Architect and/or Owner prior to proceeding. (expand to include field sample instructions)?
F. Material must be tested in accordance with ASTM E 1042 by a NVLAP accredited testing laboratory.

1.04 Submittals
A. Submit product data that the product meets or exceeds the following specified requirements.
1. Bond strength shall be greater than 100 psf per ASTM E 736.
2. Product shall be Class 1 Class A per ASTM E 84.
3. Non-corrosive per ASTM C 1149
4. Comply with 2015 IBC Section 803.12 stability requirements for interior finishes.
5. Product shall be Cradle to Cradle® Certified v.3.1 or higher to a minimum certification level of Bronze
6. Product shall be UL GREENGUARD Gold Certified
7. Product must have a publicly available Health Product Declaration (HPD) to 100 PPM
8. Product must have a third-party verified, publicly available, product-specific Environmental Product Declaration per ISO 14025
B. Manufacturer's written certification that product contains no asbestos, fiberglass or other man-made mineral fibers.
C. Copy of manufacturer’s ISO 9001:2015 Certification.
D. Minimum Fiber Recycled Content to be 75%.
E. Cannot contain any added Urea-Formaldehyde Resins.

1.06 Delivery, Storage and Handling
A. Deliver in original, unopened containers bearing name of manufacturer and product identification.
B. Store materials dry, off ground, and under cover.
C. Protect liquid adhesive from freezing.
D. Water to be potable.
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2.01 Acceptable Manufacturers
A. International Cellulose Corporation 12315 Robin Boulevard
Houston, Texas 77045
Phone: (713) 433-6701 or (800) 444-1252
Fax: (713) 433-2029
Website: www.spray-on.com Email: icc@saint-gobain.com
B. For approved applicators contact ICC at (800) 444-1252.

2.02 Materials
A. SonaKrete® Acoustical Finish System
1. Color shall be from Manufacturer’s standard color chart or custom color as noted
2. Each bag must be labeled appropriately.
3. Each drum of adhesive must be labeled “SonaKrete® Adhesive”.

PART 3 – EXECUTION
3.01 Examination
A. Examine surfaces and report unsatisfactory conditions in writing. Do not proceed until unsatisfactory conditions are corrected.
B. Verify surfaces to receive application of acoustical finish to determine if priming/sealing is required to insure bonding and/or to prevent discoloration caused by migratory stains.

3.02 Preparation
A. Provide masking, drop cloths or other satisfactory coverings for materials/surfaces that are not to receive acoustical finish to protect from over-spray.
B. Coordinate installation of the acoustical finish system with work of other trades.
C. Prime surfaces as required by manufacturer’s instructions or as determined by examination.
D. General substrate preparation may include; but is not limited, to the following:
1. Gypsum/Drywall Substrates: A minimum level 3, preferably level 4 primed finish is recommended.
2. Drywall substrates are to be primed with a suitable drywall primer such as: Sherwin Williams® Multi-Purpose Water-Based Acrylic Alkyd.
3. The use of Quickset, Quicksand, Drywall Joint Compound is not acceptable.
4. Plaster substrates may require brown coat finish.
5. Consult the manufacturer for other substrates.

3.03 Installation
A. Install acoustical finish system according to manufacturer’s recommendations.
B. Comply with local Building Code requirements.
C. Install the acoustical finish system to achieve an average NRC of 	.
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	SonaKrete® Acoustical Finish System on Solid Backing:

	Thickness:
	NRC:

	0.25”
	0.50

	0.375”
	0.55

	0.50”
	0.65

	0.75”
	0.75



Acoustical testing performed by NVLAP certified testing lab.

D. After achieving the required thickness and while still wet, float the material to match the approved field sample.
E. Cure the material with continuous natural or mechanical ventilation.
a.  Continuous ventilation must be maintained until the material has properly cured
F. Remove and dispose of over-spray.

4.01 Protection
A. Protect finished installation under provision of Division 1.
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